Four in Hand

1. Situate the tie so that the end "A" is longer than end "B" and cross "A" over "B".

4. Pull "A" up and through the loop around your neck.

2. Turn "A" back underneath "B".

5. Hold the front of the knot loosely with your index finger and bring "A" down through front loop.

3. Continue by bringing "A" back over in front of "B" again.

6. Remove finger and tighten knot snugly to collar by holding "B" and sliding the knot.